;Subttl	Drive Ogranization Definitions [Quantum 34 meg Floppy] (23_Aug_84)
;
;	Copyright (c), 1983, 1984
;	Morrow Designs, Inc.
;	600 McCormick
;	San Leandro, Ca. 94577
;
Floppy	equ	True		;True for Floppy system; False for Hard Disk
Drives	equ	5		;number of drives you wish to define
Auto	equ	True		;Auto Command Load from the Ims Buffer
;
;	1) Make sure that the floppy flag is set to FALSE for generating a
;	   loader for the hard disk.
;	2) If you're generating a loader for a floppy disk then	floppy should
;	   be set to TRUE and you MUST have entered an F argument to the end
;	   of the Boot.Sub/Bios.Sub command invocations (eg Boot F)
;	3) The currently defined drives are:
;
;	DSDD	Floppy Disk 5.25 inch double sided double density 48 tpi drive
;
;	ST06	Winchester  Seagate, Model ST506 (5 meg)
;	SA11	    "       Shugart Associates, Model SA712 (11 meg)
;	SQ06        "       SyQuest Technology, Model 306 (6 meg)
;	CM11	    "       Computer Memories Inc., Model 5412, (11 meg)
;	CM16	    "       Computer Memories Inc., Model 5619, (16 meg)
;	CM34	    "       Computer Memories Inc., Model 6640, (34 meg)
;	CD31	    "       Control Data Corporation, Model 9415-5 (31 meg)
;	MS11	    "       Mini-Scribe, Model 3212 (11 meg)
;	TU34	    "	    Tulin Corporation, Model TL 240 (34 meg)
;	QU36	    "	    Quantum Corporation, Model Q540 (36 meg)
;
; Floppy Disk Definitions
;------------------------
;
	if	floppy
cvdsk	equ	0		;first floppy is current virtual, a:
	define	a,dsdd
	define	b,QU36		;Quantum 36 meg hard disk
	define	c,dsdd
	define	d,dsdd
	define	e,dsdd
	else

; Hard Disk Definitions
;----------------------
;
cvdsk	equ	1		;first floppy is current virtual, b:
	define	a,QU36		;Quantum 36 meg hard disk
	define	b,dsdd
	define	c,dsdd
	define	d,dsdd
	define	e,dsdd
	endif
	page
